YJ USB Serial Driver r1.3 - 11/12/12
===========================================

This Youjie USB Driver package - non-Microsoft WHQL Certified, supports the following device:

1/ Handheld Barcode Scanner = VID_23D0/PID_0B94 (REM off)
                              VID_23D0/PID_0B8A (REM on)

 This driver package can coexist with the Honeywell HSM USB driver package.


Driver Installation/Uninstallation Instructions
===============================================

1/ Installation:
  A/ Windows 32 bits OS:
    * For Windows 2000, xp: Browse and double click the install file "Install_x86.bat" in the install media folder.
    * For Windows 7: Browse, right click, and select "Run as administrator" the install file "Install_x86.bat" in the install media folder.

  B/ Windows 64 bits OS:
    * For Windows xp: Browse and double click the install file "Install_x64.bat" in the install media folder.
    * For Windows 7: Browse, right click, and select "Run as administrator" the install file "Install_x64.bat" in the install media folder.

2/ Uninstallation:
  A/ Windows 32 bits OS:
    * For Windows 2000, xp: Browse and double click the install file "Uninstall_x86.bat" in the install media folder.
    * For Windows 7: Browse, right click, and select "Run as administrator" the install file "Uninstall_x86.bat" in the install media folder.

  B/ Windows 64 bits OS:
    * For Windows xp: Browse and double click the install file "Uninstall_x64.bat" in the install media folder.
    * For Windows 7: Browse, right click, and select "Run as administrator" the install file "Uninstall_x64.bat" in the install media folder.